!!!Note:

1. The Bluetooth module needs to be properly inserted into the expansion board of the robot car.

2. 51/Arduino Download Switch on the expansion board must be set to [OFF].

3. The ultrasonic module must be inserted.